
FLUKE USB SERIAL DRIVER INSTALLATION                         V1.00.0000 7/2013
==============================================================================

This directory contains the necessary files to install the Fluke
USB serial driver. When installed, the driver allows a Windows PC to
communicate with the product using its USB remote port over a virtual
COM port.

1.	Turn on the Fluke product.

2.	Using Windows Explorer, select one of these programs:

	Fluke_USB_Serial_Driver_x64.exe	for 64 bit versions of Windows
	Fluke_USB_Serial_Driver_x86.exe for 32 bit versions of Windows

3.	Follow the instructions given by the installer.

4.	Connect the Fluke product to the PC with a USB cable.

5.	Select "USB" as the "Active Remote Port" for the product.

6.	Use the new COM port added to the PC to communicate with
	the product.

If the USB driver does not install properly, please contact Fluke
Technical Support at (800)44-FLUKE, or via the Fluke website at
http://www.fluke.com.

